**KH – 88 Metal Seated**

**Mining Solid Medium**

**KH – 64 K, Top Entry Design**

**KH – 67 K, Top Entry Design**

**KH – 80 Metal / Soft Seated**

**KH – 85 Metal / Soft Seated**

**KH – 75 Metal / Soft Seated**

**KH – 20 Soft Seated**

**KH – 21 Metal / Soft Seated**

**KH – 25 Metal / Soft Seated**

**KH – 23 Metal / Soft Seated**

**KH – 24 Metal / Soft Seated**

**General Chemicals**

**KH – 16 Metal / Soft Seated**

**KH – 22 Metal / Soft Seated**

**KH – 70 Metal / Soft Seated**

**KH – 15 Metal / Soft Seated**

**KH – 14 Metal / Soft Seated**

**KH – 11 Soft Seated**

**Nuclear Power**

**Cryogenic**

**Vaccum Service**

**All Round**

**Polypropylene / PE**

**PTA / Pharmaceuticals**

**Tank Bottom Drain**

**Application**

**Ball Valves**